AVRDUDE: Programmer Definitions

[ < ] | [ > ] |  | [ << ] | [ Up ] | [ >> ] |  |  |  |  | [Top] | [Contents] | [Index] | [ ? ]

## 4.2 Programmer Definitions

The format of the programmer definition is as follows:

    programmer
        id     = <id1> [, <id2> [, <id3>] ...] ;  # <idN> are quoted strings
        desc     = <description> ;                  # quoted string
        type     = par | stk500 ;                   # programmer type
        baudrate = <num> ;                          # baudrate for serial ports
        vcc      = <num1> [, <num2> ... ] ;         # pin number(s)
        reset    = <num> ;                          # pin number
        sck      = <num> ;                          # pin number
        mosi     = <num> ;                          # pin number
        miso     = <num> ;                          # pin number
        errled   = <num> ;                          # pin number
        rdyled   = <num> ;                          # pin number
        pgmled   = <num> ;                          # pin number
        vfyled   = <num> ;                          # pin number
      ;

This document was generated by root on January, 24 2006 using texi2html