AVRDUDE: Part Definitions

[ < ] | [ > ] |  | [ << ] | [ Up ] | [ >> ] |  |  |  |  | [Top] | [Contents] | [Index] | [ ? ]

## 4.3 Part Definitions

    part
        id               = <id> ;                 # quoted string
        desc             = <description> ;        # quoted string
        devicecode       = <num> ;                # numeric
        chip_erase_delay = <num> ;                # micro-seconds
        pagel            = <num> ;                # pin name in hex, i.e., 0xD7
        bs2              = <num> ;                # pin name in hex, i.e., 0xA0
        reset            = dedicated | io;
        retry_pulse      = reset | sck;
        pgm_enable       = <instruction format> ;
        chip_erase       = <instruction format> ;
        memory <memtype>
            paged           = <yes/no> ;          # yes / no
            size            = <num> ;             # bytes
            page_size       = <num> ;             # bytes
            num_pages       = <num> ;             # numeric
            min_write_delay = <num> ;             # micro-seconds
            max_write_delay = <num> ;             # micro-seconds
            readback_p1     = <num> ;             # byte value
            readback_p2     = <num> ;             # byte value
            pwroff_after_write = <yes/no> ;       # yes / no
            read            = <instruction format> ;
            write           = <instruction format> ;
            read_lo         = <instruction format> ;
            read_hi         = <instruction format> ;
            write_lo        = <instruction format> ;
            write_hi        = <instruction format> ;
            loadpage_lo     = <instruction format> ;
            loadpage_hi     = <instruction format> ;
            writepage       = <instruction format> ;
          ;
      ;

> 4.3.1 Instruction Format |  |

This document was generated by root on January, 24 2006 using texi2html