AVRDUDE: Option Descriptions

[ < ] | [ > ] |  | [ << ] | [ Up ] | [ >> ] |  |  |  |  | [Top] | [Contents] | [Index] | [ ? ]

## 2.1 Option Descriptions

AVRDUDE is a command line tool, used as follows:

    avrdude -p partno options ...

Command line options are used to control AVRDUDE's behaviour. The following options are recognized:

`-p partno`
  This is the only mandatory option and it tells AVRDUDE what type of part (MCU) that is connected to the programmer. The partno parameter is the part's id listed in the configuration file. Specify -p ? to list all parts in the configuration file. If a part is unknown to AVRDUDE, it means that there is no config file entry for that part, but it can be added to the configuration file if you have the Atmel datasheet so that you can enter the programming specifications. Currently, the following MCU types are understood:

  `c128`
    AT90CAN128

  `pwm2`
    AT90PWM2

  `pwm3`
    AT90PWM3

  `1200`
    AT90S1200

  `2313`
    AT90S2313

  `2333`
    AT90S2333

  `2343`
    AT90S2343 (*)

  `4414`
    AT90S4414

  `4433`
    AT90S4433

  `4434`
    AT90S4434

  `8515`
    AT90S8515

  `8535`
    AT90S8535

  `m103`
    ATmega103

  `m128`
    ATmega128

  `m1280`
    ATmega1280

  `m1281`
    ATmega1281

  `m16`
    ATmega16

  `m161`
    ATmega161

  `m162`
    ATmega162

  `m163`
    ATmega163

  `m164`
    ATmega164

  `m169`
    ATmega169

  `m32`
    ATmega32

  `m324`
    ATmega324

  `m329`
    ATmega329

  `m3290`
    ATmega3290

  `m48`
    ATmega48

  `m64`
    ATmega64

  `m640`
    ATmega640

  `m644`
    ATmega644

  `m649`
    ATmega649

  `m6490`
    ATmega6490

  `m8`
    ATmega8

  `m8515`
    ATmega8515

  `m8535`
    ATmega8535

  `m88`
    ATmega88

  `t12`
    ATtiny12

  `t13`
    ATtiny13

  `t15`
    ATtiny15

  `t2313`
    ATtiny2313

  `t25`
    ATtiny25

  `t26`
    ATtiny26

  `t45`
    ATtiny45

  `t85`
    ATtiny85

  (*) The AT90S2323 and ATtiny22 use the same algorithm.

`-b baudrate`
  Override the RS-232 connection baud rate specified in the respective programmer's entry of the configuration file.

`-B bitclock`
  Specify the bit clock period for the JTAG interface (JTAG ICE only). The value is a floating-point number in microseconds. The default value of the JTAG ICE results in about 1 microsecond bit clock period, suitable for target MCUs running at 4 MHz clock and above. Unlike certain parameters in the STK500, the JTAG ICE resets all its parameters to default values when the programming software signs off from the ICE, so for MCUs running at lower clock speeds, this parameter must be specified on the command-line.

`-c programmer-id`
  Specify the programmer to be used. AVRDUDE knows about several common programmers. Use this option to specify which one to use. The programmer-id parameter is the programmer's id listed in the configuration file. Specify -c ? to list all programmers in the configuration file. If you have a programmer that is unknown to AVRDUDE, and the programmer is controlled via the PC parallel port, there's a good chance that it can be easily added to the configuration file without any code changes to AVRDUDE. Simply copy an existing entry and change the pin definitions to match that of the unknown programmer. Currently, the following programmer ids are understood and supported:

  `abcmini`
    ABCmini Board, aka Dick Smith HOTCHIP

  `alf`
    Nightshade ALF-PgmAVR, http://nightshade.homeip.net/

  `avr109`
    Atmel AppNote AVR109 Boot Loader

  `avr910`
    Atmel Low Cost Serial Programmer

  `avr911`
    Atmel AppNote AVR911 AVROSP (an alias for avr109)

  `avrisp`
    Atmel AVR ISP (an alias for stk500)

  `avrispv2`
    Atmel AVR ISP, running a version 2.x firmware (an alias for stk500v2)

  `avrispmkII`
    Atmel AVR ISP mkII (alias for stk500v2)

  `avrispmk2`
    Atmel AVR ISP mkII (alias for stk500v2)

  `bascom`
    Bascom SAMPLE programming cable

  `bsd`
    Brian Dean's Programmer, http://www.bsdhome.com/avrdude/

  `butterfly`
    Atmel Butterfly Development Board

  `dt006`
    Dontronics DT006

  `jtagmkI`
  `jtag1`
    Atmel JTAG ICE mkI, running at 115200 Bd

  `jtag1slow`
    Atmel JTAG ICE mkI, running at 19200 Bd

  `jtagmkII`
  `jtag2slow`
    Atmel JTAG ICE mkII (default speed 19200 Bd)

  `jtag2fast`
    Atmel JTAG ICE mkII, running at 115200 Bd

  `jtag2`
    Same as before.

  `pavr`
    Jason Kyle's pAVR Serial Programmer

  `picoweb`
    Picoweb Programming Cable, http://www.picoweb.net/

  `pony-stk200`
    Pony Prog STK200

  `sp12`
    Steve Bolt's Programmer

  `stk200`
    STK200

  `stk500`
    Atmel STK500

  `stk500v2`
    Atmel STK500, running a version 2.x firmware

`-C config-file`
  Use the specified config file for configuration data. This file contains all programmer and part definitions that AVRDUDE knows about. If you have a programmer or part that AVRDUDE does not know about, you can add it to the config file (be sure and submit a patch back to the author so that it can be incorporated for the next version). If not specified, AVRDUDE reads the configuration file from /usr/local/etc/avrdude.conf (FreeBSD and Linux). See Appendix A for the method of searching for the configuration file for Windows.

`-D`
  Disable auto erase for flash. When the -U option with flash memory is specified, avrdude will perform a chip erase before starting any of the programming operations, since it generally is a mistake to program the flash without performing an erase first. This option disables that. However, to remain backward compatible, the -i, and -m options automatically disable the auto erase feature.

`-e`
  Causes a chip erase to be executed. This will reset the contents of the flash ROM and EEPROM to the value `0xff', and is basically a prerequisite command before the flash ROM can be reprogrammed again. The only exception would be if the new contents would exclusively cause bits to be programmed from the value `1' to `0'. Note that in order to reprogram EERPOM cells, no explicit prior chip erase is required since the MCU provides an auto-erase cycle in that case before programming the cell.

`-E exitspec[,...]`
  By default, AVRDUDE leaves the parallel port in the same state at exit as it has been found at startup. This option modifies the state of the `/RESET' and `Vcc' lines the parallel port is left at, according to the exitspec arguments provided, as follows:

  `reset`
    The `/RESET' signal will be left activated at program exit, that is it will be held low, in order to keep the MCU in reset state afterwards. Note in particular that the programming algorithm for the AT90S1200 device mandates that the `/RESET' signal is active before powering up the MCU, so in case an external power supply is used for this MCU type, a previous invocation of AVRDUDE with this option specified is one of the possible ways to guarantee this condition.

  `noreset`
    The `/RESET' line will be deactivated at program exit, thus allowing the MCU target program to run while the programming hardware remains connected.

  `vcc`
    This option will leave those parallel port pins active (i. e. high) that can be used to supply `Vcc' power to the MCU.

  `novcc`
    This option will pull the `Vcc' pins of the parallel port down at program exit.

  Multiple exitspec arguments can be separated with commas.

`-F`
  Normally, AVRDUDE tries to verify that the device signature read from the part is reasonable before continuing. Since it can happen from time to time that a device has a broken (erased or overwritten) device signature but is otherwise operating normally, this options is provided to override the check.

`-n`
  No-write - disables actually writing data to the MCU (useful for debugging AVRDUDE).

`-P port`
  Use port to identify the device to which the programmer is attached. Normally, the default parallel port is used, but if the programmer type normally connects to the serial port, the default serial port will be used. See Appendix A, Platform Dependent Information, to find out the default port names for your platform. If you need to use a different parallel or serial port, use this option to specify the alternate port name.

  For the JTAG ICE mkII, if AVRDUDE has been built with libusb support, port may alternatively be specified as usb[:serialno]. In that case, the JTAG ICE mkII will be looked up on USB. If serialno is also specified, it will be matched against the serial number read from any JTAG ICE mkII found on USB. The match is done after stripping any existing colons from the given serial number, and right-to-left, so only the least significant bytes from the serial number need to be given. For a trick how to find out the serial numbers of all JTAG ICEs attached to USB, see 2.2 Example Command Line Invocations.

  As the AVRISP mkII device can only be talked to over USB, the very same method of specifying the port is required there.

`-q`
  Disable (or quell) output of the progress bar while reading or writing to the device. Specify it a second time for even quieter operation.

`-u`
  Disables the default behaviour of reading out the fuses three times before programming, then verifying at the end of programming that the fuses have not changed. If you want to change fuses you will need to specify this option, as avrdude will see the fuses have changed (even though you wanted to) and will change them back for your "saftey". This option was designed to prevent cases of fuse bits magically changing (usually called safemode).

`-t`
  Tells AVRDUDE to enter the interactive "terminal" mode instead of up- or downloading files. See below for a detailed description of the terminal mode.

`-U memtype:op:filename[:format]`
  Perform a memory operation, equivalent to specifing the ``-m'`, ``-i'` or ``-o'`, and ``-f'` options, except that multiple ``-U'` optins can be specified in order to operate on mulitple memories on the same command-line invocation. The memtype field specifies the memory type to operate on. Use the ``-v'` option on the command line or the `part` command from terminal mode to display all the memory types supported by a particular device. Typically, a device's memory configuration at least contains the memory types `flash` and `eeprom`. All memory types currently known are:
  `calibration`
    One or more bytes of RC oscillator calibration data.
  `eeprom`
    The EEPROM of the device.
  `efuse`
    The extended fuse byte.
  `flash`
    The flash ROM of the device.
  `fuse`
    The fuse byte in devices that have only a single fuse byte.
  `hfuse`
    The high fuse byte.
  `lfuse`
    The low fuse byte.
  `lock`
    The lock byte.
  `signature`
    The three device signature bytes (device ID).

  The op field specifies what operation to perform:

  `r`
    read the specified device memory and write to the specified file

  `w`
    read the specified file and write it to the specified device memory

  `v`
    read the specified device memory and the specified file and perform a verify operation

  The filename field indicates the name of the file to read or write. The format field is optional and contains the format of the file to read or write. Possible values are:

  `i`
    Intel Hex

  `s`
    Motorola S-record

  `r`
    raw binary; little-endian byte order, in the case of the flash ROM data

  `m`
    immediate mode; actual byte values specified on the command line, seperated by commas or spaces in place of the filename field of the ``-i'`, ``-o'`, or ``-U'` options. This is useful for programming fuse bytes without having to create a single-byte file or enter terminal mode. If the number specified begins with `0x`, it is treated as a hex value. If the number otherwise begins with a leading zero (`0`) it is treated as octal. Otherwise, the value is treated as decimal.

  `a`
    auto detect; valid for input only, and only if the input is not provided at stdin.

  The default is to use auto detection for input files, and raw binary format for output files.

  Note that if filename contains a colon, the format field is no longer optional since the filename part following the colon would otherwise be misinterpreted as format.

`-v`
  Enable verbose output.

`-V`
  Disable automatic verify check when uploading data.

`-y`
  Tells AVRDUDE to use the last four bytes of the connected parts' EEPROM memory to track the number of times the device has been erased. When this option is used and the ``-e'` flag is specified to generate a chip erase, the previous counter will be saved before the chip erase, it is then incremented, and written back after the erase cycle completes. Presumably, the device would only be erased just before being programmed, and thus, this can be utilized to give an indication of how many erase-rewrite cycles the part has undergone. Since the FLASH memory can only endure a finite number of erase-rewrite cycles, one can use this option to track when a part is nearing the limit. The typical limit for Atmel AVR FLASH is 1000 cycles. Of course, if the application needs the last four bytes of EEPROM memory, this option should not be used.

`-Y cycles`
  Instructs AVRDUDE to initialize the erase-rewrite cycle counter residing at the last four bytes of EEPROM memory to the specified value. If the application needs the last four bytes of EEPROM memory, this option should not be used.

[ < ] | [ > ] |  | [ << ] | [ Up ] | [ >> ] |  |  |  |  | [Top] | [Contents] | [Index] | [ ? ]

This document was generated by root on January, 24 2006 using texi2html